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	SECTION I:  GENERAL INFORMATION

	*Product Identification:
(Reference #)  EnviroRite Mold, Mildew & Bacteria Detergent Disinfectant Spray

Product Class:   Nonionic/quaternary blend

*Precautions:   Severely irritating to skin & eyes

	Section II:  Hazardous Ingredients/CAS #
	%
	ACGIH TWA

	None
	
	

	Section IIA:  Hazardous By-Products
	
	

	None
	
	

	SECTION III:  PHYSICAL DATA

	Flash Point:  200°F (Method = 16~) Setaflash
	Vapor Pressure:  N.D.  (mm Hg)

	Boiling Point:  200°F

	pH:  (mm Hg)  11.7 as is

	Volatiles:
9.3% (by Weight) 


(Volatile = Boiling Point  400°F)
	Density:  8.0 (lbs/gal)

	Evaporation:  Slower than Ethyl Ether
	Solubility in Water:  Complete

	Vapor Density:  Heavier Than Air

	Appearance @ 70°F:  Clear liquid

	
N.D. = Not Determined
N.A.= Not Applicable

	SECTION IV: FIRE, EXPLOSION AND REACTIVITY DATA

	Extinguishing Media:
	CO2, Dry Chemicals, Synthetic Foam or Water.  Type BC or ABC Extinguishers.

	Unusual Fire & Explosion Hazards:
	Strong acids and bases react with aluminum to form hydrogen which is explosive if ignited.  Dust may present an explosion hazard.  Fluorocarbons will develop pressure in containers heated above 75°F.

	Special Fire Fighting Procedures:
	Use self-contained breathing apparatus for maximum respiratory protection.  Water may be used to cool containers if not ruptured or leaking.

	Stability:
	Stable.

	Incompatibility:  (Materials to Avoid)
	Anionic materials, strong oxidizers.

	Hazardous Decomposition Products:
	Nitrous oxides, ammonical vapors.

	SECTION V:  HEALTH HAZARD DATA

	Effects of Exposure:
	Contact with eyes causes irritation.  Prolonged or repeated contact with skin may cause irritation.  Dusts, vapors, or mists may irritate respiratory passages.  If corrosive, (see Section 1), contact may cause chemical burns.  If alcohol or other solvents are present above TLV, (see Section 2), vapors may cause drowsiness, nausea, loss of motor skills, or disorientation.

	Emergency and First Aid Precautions:

	Eye Contact:
	Flush eyes immediately with plenty of water for at least 15 minutes.

	Skin Contact:
	Wash off skin and remove contaminated clothing.  Do not reuse contaminated clothing.

	Inhalation:
	If dust, vapors, or mist cause distress, remove to fresh air.  Use oxygen or artificial respiration, if needed.

	Ingestion:
	If swallowed, consult a physician immediately. 



	
If Symptoms Persist, Consult A Physician.


	SECTION VI:  ENVIRONMENTAL PROTECTION

	Spill & Leak Response Procedure:

· Contain all spills and leaks to prevent discharge to the environment.

· Ventilate area.

· If flammable or combustible, (see Section 1), avoid spark, fires and open flames, and use non-sparking equipment.

· If strong acid, (see Section 3), carefully neutralize with lime, sodium carbonate or sodium bicarbonate.


Small Spill:
Soak up with absorbent.  Shovel into waste containers.  Flush area with water.


Large Spill:
Recover spilled material for reprocessing or disposal.
Waste Disposal Method:
Recover liquid or dispose waste material, (incineration is preferred), in accordance with all applicable federal, state, and local regulations and laws.  Material collected with absorbent may be disposed of in a permitted landfill in accordance with all applicable federal, state and local regulations and laws.



	SECTION VII:  SPECIAL PROTECTION INFORMATION

	Eye Protection:
Wear goggles or full face shield when handling to avoid contact with face or eyes.

Ventilation:   Provide adequate ventilation.  Keep hazardous ingredients below their TLV.

Other Protective Equipment:
Use impervious gloves and any other  protective equipment to prevent prolonged or repeated contact.

Respiratory Protection:
If vapors, fumes, or dusts are present use a MSHA or NIOSH approved respirator, a fresh air breathing apparatus, or a self-contained breathing apparatus.



	SECTION VIII:  SPECIAL PRECAUTIONS

	Handling and Storage:
Avoid overheating or freezing.  (See Section 3).  Store in a cool, well-ventilated area.  If flammable or combustible, (see Section 1), avoid sparks, fires, and open flames.  Ground equipment when transferring or using material.

Do Not Take Internally!

If Ingested, Call A Physician!

Do Not Inhale Vapors, Fumes, Or Dusts!

Wash Thoroughly After Handling!

Spilled Material Is Slippery!



	SECTION IX:  DISCLAIMER

	Neither this data sheet nor any statement contained herein grants or extends any license express or implied, in connection with patents issued or pending which may be the property of the manufacturer or others.  The information in this data sheet has been assembled by the manufacturer based on its own study and on the work of others.  The manufacturer makes no warranties, expressed or implied, as to the accuracy, completeness, or adequacy of the information contained herein.  The manufacturer shall not be liable (regardless of fault) to the vendee, the vendee’s employees, or anyone for any direct, special, or consequential damages arising out of or in connection with the accuracy, completeness, adequacy, or furnishing of such information.
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* Label Information
** Registered Trademark or Application Pending


